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	Purpose:
To outline the procedure for safely and correctly installing an air conditioner in a caravan.

	Procedure:
· Step 1: Inspect the roof for correct installation procedure and clean the surface using a rag.
· Step 2: Mark the mounting points on the roof for the brackets and drill holes for the bracket. Make sure not to damage any wires or insulation.
· Step 3: Secure the mounting brackets using Tek screws and bolts using a torque wrench to 10Nm (Recommended Spec).
· Step 4: Lift and place the air con unit on the roof and secure it to the brackets using the provided bolts.
· Step 5: Apply SMP 50 silicone sealant around the base of the air con to prevent any leakage. 
· Step 6: Wipe out any extra silicone residue and check for the seals to ensure they are tight and smooth
· Step 7: Connect the air conditioner wires to the electrical systems and test the connection.
· Step 8: Turn on the air conditioner to check if it is working properly.
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	Reference Document (if any): 
· Air conditioner installation manual

	Roles and Responsibilities: 

	Role:
Production Operator (Roof section)
	Responsibilities:
Ensure the assembly steps are followed precisely, inspect parts for defects, and document any discrepancies.

	Required Tools and Equipment:
· Power tools
· Sealants (SMP 50)
· Mounting brackets
· Ladder
· Silicon gun
· Torque wrench

	PPE:
· Safety glass
· Ear plug
· Safety gloves
· Steel caped boot
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